



**Model 8700 RV/Car Haul Trailers**





**The Model 8700 trailer is manufactured with a structural heavy duty steel frame, huck bolt fastened steel crossmembers, poonched steel tread loading deck and a fully enclosed steel center deck. The trailer weighs 9,100 lbs. and can be rated up to 32,000 GVWR and is an easy tow behind a 1-1/2 ton or better pickup truck or a semi tractor as dependent on the trailer rating.**

## Standard Features:

53’ x 102” RV Trailer Structural Steel Frame

4” Steel Channel Crossmember Supports

Huck Bolt Structural Fasteners Used On All Critical Joints

Steel Poonched Loading Deck and Rub-Rail

Fully Enclosed Steel Center Deck w/ Flush Center Rail

1. 10,000 lb. Axles (26,000 GVWR)

235/75R17.5 - 16 Ply Radial Tires and Steel Wheels

235/75R17.5 - 16 Ply Radial Spare Tire w/ Carrier

Electric Over Hydraulic Disc Brake Controller Kit

Paint - Black Two Component Alkyd Topcoat Over Primer

Front Track ‘Stinger’ Extension

Single Battery in Dedicated Aluminum Controls Box

Electric Planetary Gear Winch with Wireless Remote

1. RV Electrical Receptacles Front, Mid and Rear Trailer

Seven Pin RV Tow Vehicle Connecting Plug w/ 6 ft. Wire Lead

Std. Two Pin Forklift Plug for Charging Electric Winch

25,000 lb. Landing Gear

LED Lighting

34” Over Wheel Deck Height

(2) 48”x18”x18” Lockable Aluminum Toolboxes

1. Set of Aluminum Front Jump Ramps

(1) Set of 10 ft. Aluminum Loading Ramps

(3) Ball Tower

(1) Wheel Tower

(12) Ratchet Straps with Double Deck Hook Ends

DOT Conspicuity Reflective Tape

DOT Inspection

1 Year Manufacturer’s Warranty

**Optional Features:**

Aluminum Poonched Decking

Aluminum Center Deck

Aluminum Wheels (each)

Additional Spare Tire & Carrier (each)

(2) 15,000 lb. Axles (32,000 GVWR)

(1) 20,000 lb. Dual Tire Air Ride Axle (26,000 GVWR)

(2) 20,000 lb. Dual Tire Air Ride Axle (36,000 GVWR)

Custom Paint Color (other than standard black)

Additional 48” Aluminum Toolbox (each)

Additional 48” Steel Toolbox (each)

Additional Battery in Toolbox

12 V 12,000 lb. Worm Drive Winch

LED Lights (each)

**KANN Manufacturing Corporation**

210 Regent Street

PO Box 400

Guttenberg, IA 52052

P. 800.806.5266 F. 563.252.3069

[www.kannmfg.com](http://www.kannmfg.com/) [www.facebook.com/kannmfg](http://www.facebook.com/kannmfg)

For more information please contact:

Email: [sales@kannmfg.com](mailto:sales@kannmfg.com)

Phone: 800-806-5266 ext. 211